

Installation Notes from Clemens Szyperski

1.Boot Oberon

2. Diskette.ReadAll

on both “Oberon Master” floppy disks

(Nr. 2 only contains support

for the Color Screen – can be omitted)

3. Boot Medos-2

4. Files SEK.ABS, OberonBoot.ABS

-> copy from “Medos-2 to Oberon”

to PC.BootFile0/1

In Oberon, now delete:

 Display\*

 \*obj \*sym \*ref

 ^ ^ ^ all lower-case letters